{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Simple Boiler","Incinerator"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Simple Boiler","index":0,"n_rows":50,"n_cols":16,"rows_kept":50,"cut":false,"hidden":false,"merged":[]}
[]
[null,"The tables are free and provided as is. We take no responsibilities for any errors in the code or damage thereby."]
[]
[null,"Fuel",null,{"$f":"_xll.alera(\"TX0218FUEL01\",C6,C13,C15,C16,C17,C18,C19,C20)","v":"Link"},null,"Comb.",null,{"$f":"_xll.alera(\"TX0218COMB02\",G8,G18,G20,G21,G22,G24,G23,,,,,,,,,F27,F28)","v":"Link"},null,"Heat Exchanger",null,{"$f":"_xll.alera(\"TX0218HEXX02\",K21,,,,,,,,,,,,,,,,,J23,J24)","v":"Link"},null,"Final T",null,{"$f":"_xll.alera(\"TX0218HEXX03\",O19,O21,,,,,,,,,,,,,,,,N24)","v":"Link"}]
[null,"F00020000"]
[null,"H2O",50,"%",null,"Heat",9.0152788042220404,{"$f":"_xll.aleraTX(\"TX0554TXCOMBX1\")","v":"MW net"},null,"Heat",2.0801166374682962,{"$f":"_xll.aleraTX(\"TX0554TXHEXX02\")","v":"MW net"},null,"Heat",2.0801166374682962,{"$f":"_xll.aleraTX(\"TX0554TXHEXX03\")","v":"MW net"}]
[null,null,null,null,null,"Exit gas",1024.858750204872,"°C",null,"Exit gas",279.99855065255883,"°C",null,"Exit gas",279.99855065255883,"°C"]
[null,"LCV",8.0139398500000016,{"$f":"_xll.aleraTX(\"TX0550TXFUELBX\")","v":"MJ/kg"},null,null,null,7.6323236666666663,null,"Input",1024.858750204872,"°C",null,"Input",279.99855065255883,"°C"]
[null,"G 6",null,null,null,"gas",18141.132715480864,"Nm3/h",null,"gas",18141.132715480864,"Nm3/h",null,"gas",18141.132715480864,"Nm3/h"]
[null,"dry",null,null,null,null,22312.666583582701,"kg/h",null,null,22312.666583582701,"kg/h",null,null,22312.666583582701,"kg/h"]
[null,"C",47.480000000000004,"%",null,null,"Vol(wet) %",null,null,null,"Vol(wet) %",null,null,null,"Vol(wet) %"]
[null,"H",7.1200000000000019,"%",null,"N2",61.488221945038823,null,null,"N2",61.488221945038823,null,null,"N2",61.488221945038823]
[null,"N",1,"%",null,"CO2",9.7400133472086718,null,null,"CO2",9.7400133472086718,null,null,"CO2",9.7400133472086718]
[null,"O",42.20000000000001,"%",null,"H2O",23.39424982135542,null,null,"H2O",23.39424982135542,null,null,"H2O",23.39424982135542]
[null,"S",0.2,"%",null,"O2",5.3624025125051222,null,null,"O2",5.3624025125051222,null,null,"O2",5.3624025125051222]
[null,"ash",2,"%",null,"SO2",1.511237389196411E-2,null,null,"SO2",1.511237389196411E-2,null,null,"SO2",1.511237389196411E-2]
[null,"Cl",0,"%",null,"HCl",0,null,null,"HCl",0,null,null,"HCl",0]
[null,"F",0,"%",null,"O2 (dry)",7,"%",null,null,0,null,null,null,0]
[null,"O/C",0.88879528222409443,"(mass)",null,"Air",14253.642876299944,"Nm3/h",null,null,null,null,null,"Exit gas",280,"°C"]
[null,"H/C",0.14995787700084248,"(mass)",null,"base",15,"°C"]
[null,null,null,null,null,"heated",15,"°C",null,"Loss",3,"%"]
[null,null,null,null,null,"H2O",7,"g/kg"]
[null,null,null,null,null,"Fuel",4226.2221606300027,"kg/h",null,{"$f":"L33","v":"Link"},"Link to user",null,null,{"$f":"H4","v":"Link"},"Comb."]
[null,null,null,null,null,"Loss",5,"%",null,{"$f":"H4","v":"Link"},"Link to Gas",null,null,{"$f":"L4","v":"Link"},"Link to Gas"]
[]
[null,null,null,null,null,null,"Link to R - Gas",null,null,"Counter Flow",null,{"$f":"_xll.alera(\"TX0218KXAX01\",,,,,,,,,,,,,,,,,,,J30,J31)","v":"Link"}]
[null,null,null,null,null,null,"Extra gas",null,null,"dTLog",291.35953746205223,{"$f":"_xll.aleraTX(\"TX0558TXKXAX01\")","v":"°C"}]
[null,null,null,null,null,{"$f":"D4","v":"Link"},"Link to Fuel",null,null,"K x A",23088.680605237772]
[]
[null,null,null,null,null,null,null,null,null,{"$f":"L4","v":"Link"},"Exchanger 1"]
[null,null,null,null,null,null,null,null,null,{"$f":"L33","v":"Link"},"Exchanger 2"]
[]
[null,null,null,null,null,null,null,null,null,"Saturated",null,{"$f":"_xll.alera(\"TX0218STEM02\",K41,,,,,,,,,,,,,,,,,,J46)","v":"Link"},null,"Feed Water",null,{"$f":"_xll.alera(\"TX0218STEM01\",O37,O39,O40,,,,,,,,,,,,,,,,)","v":"Link"}]
[]
[null,null,null,null,null,null,null,null,null,"Q out",7.779250461086245,{"$f":"_xll.aleraTX(\"TX0554TXSTEM02\")","v":"MW net"},null,"Q out",1.0521431593351123,{"$f":"_xll.aleraTX(\"TX0554TXSTEM01\")","v":"MW net"}]
[null,null,null,null,null,null,null,null,null,"used",6.7271073017511327,"MW"]
[null,null,null,null,null,null,null,null,null,"Flow",10000,"kg/h",null,"Flow",10000,"kg/h"]
[null,null,null,null,null,null,null,null,null,"T in",90,"°C"]
[null,null,null,null,null,null,null,null,null,"T exit",217.35577842912809,"°C",null,"T exit",90,"°C"]
[null,null,null,null,null,null,null,null,null,"Press.",null,null,null,"Press.",24,"bar (a)"]
[null,null,null,null,null,null,null,null,null,"used",22,"bar (a)",null,"used",24,"bar (a)"]
[null,null,null,null,null,null,null,null,null,"Enth.",2800.5301659910483,"kJ/kg",null,"Enth.",378.77153736064037,"kJ/kg"]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,{"$f":"P33","v":"Link"},"Link to Boiler"]
[]
[null,null,null,null,null,null,null,null,null,"Heat exchanger area"]
[null,null,null,null,null,null,null,null,null,"K",80,"W/m2K"]
[null,null,null,null,null,null,null,null,null,"A",{"$f":"K35*1000000/K49/K27","v":333.7478896713414},"m2"]

{"sheet":"Incinerator","index":1,"n_rows":52,"n_cols":36,"rows_kept":52,"cut":false,"hidden":false,"merged":[]}
[]
[null,"The tables are free and provided as is. We take no responsibilities for any errors in the code or damage thereby."]
[null,null,null,null,null,null,null,null,null,20,"%"]
[null,"Sewage Sludge",null,null,null,"In Bed Combustion",null,null,null,"Freeboard Combustion",null,null,null,"Furnace Exit",null,null,null,"Air Preheater Freebord",null,null,null,"Convective Evaporator",null,null,null,"Air Preheater Bed",null,null,null,"Economiser "]
[null,"Fuel",null,{"$f":"_xll.alera(\"TX0218FUEL05\",C7,C9,C14,C16,C17,C18,C19,C20,C21)","v":"Link"},null,"Comb.",null,{"$f":"_xll.alera(\"TX0218COMB02\",G9,G19,G21,G22,G23,G25,G24,,,,,,,,,F28,F29)","v":"Link"},null,"Comb.",null,{"$f":"_xll.alera(\"TX0218COMB02\",K9,K19,K21,K22,K23,K25,K24,,,,,,,,,J28,J29)","v":"Link"},null,"Gas Mix Box",null,{"$f":"_xll.alera(\"TX0218GASM01\",,,,,,,,,,,,,,,,,,N21,N20,)","v":"Link"},null,"Heat Exchanger",null,{"$f":"_xll.alera(\"TX0218HEXX02\",S22,,,,,,,,,,,,,,,,,R24,R25)","v":"Link"},null,"Heat Exchanger",null,{"$f":"_xll.alera(\"TX0218HEXX02\",W22,,,,,,,,,,,,,,,,,V24,V25)","v":"Link"},null,"Heat Exchanger",null,{"$f":"_xll.alera(\"TX0218HEXX02\",AA22,,,,,,,,,,,,,,,,,Z24,Z25)","v":"Link"},null,"Heat Exchanger",null,{"$f":"_xll.alera(\"TX0218HEXX02\",AE22,,,,,,,,,,,,,,,,,AD24,AD25)","v":"Link"},null,"Dew point (DP)",null,{"$f":"_xll.alera(\"TX0218HUMI01\",AI7,AI12,,,,,,,,,,,,,,,,,AH15)","v":"Link"}]
[null,"F00000004"]
[null,"H2O",63.18,"%",null,"Heat",2.6079808763600161,{"$f":"_xll.aleraTX(\"TX0554TXCOMBX1\")","v":"MW net"},null,"Heat",0.75758093654434966,{"$f":"_xll.aleraTX(\"TX0554TXCOMBX1\")","v":"MW net"},null,"Heat",3.3655618129043656,{"$f":"_xll.aleraTX(\"TX0554TXGASM01\")","v":"MW net"},null,"Heat",3.1738863924491034,{"$f":"_xll.aleraTX(\"TX0554TXHEXX02\")","v":"MW net"},null,"Heat",1.3004081981248965,{"$f":"_xll.aleraTX(\"TX0554TXHEXX02\")","v":"MW net"},null,"Heat",0.95196815036358906,{"$f":"_xll.aleraTX(\"TX0554TXHEXX02\")","v":"MW net"},null,"Heat",0.73033242872858639,{"$f":"_xll.aleraTX(\"TX0554TXHEXX02\")","v":"MW net"},null,"ambient",1013.25,{"$f":"_xll.aleraTX(\"TX0598TXHUMI01\")","v":"mbar"}]
[null,null,null,null,null,"Exit gas",786.7949965079589,"°C",null,"Exit gas",770.19341673991937,"°C",null,"Exit gas",782.99827746665687,"°C",null,"Exit gas",744.49516218561007,"°C",null,"Exit gas",338.38067386195019,"°C",null,"Exit gas",253.53195065770262,"°C",null,"Exit gas",197.39559007958928,"°C",null,"DP",68.201559797613527,"°C"]
[null,"LCV",3.53,{"$f":"_xll.aleraTX(\"TX0550TXFUELBX\")","v":"MJ/kg"},null,null,null,3.3619047619047615,null,null,null,3.3619047619047615,null,null,null,null,null,"Input",782.99827746665687,"°C",null,"Input",744.49516218561007,"°C",null,"Input",338.38067386195019,"°C",null,"Input",253.53195065770262,"°C",null,"Humidity",1.9603879564221405,"%"]
[null,"G 4",3.5308690715822091,"MJ/kg",null,"gas",7070.846032900452,"Nm3/h",null,"gas",2146.6733920478109,"Nm3/h",null,"gas",9217.5194249482629,"Nm3/h",null,"gas",9217.5194249482629,"Nm3/h",null,"gas",9217.5194249482629,"Nm3/h",null,"gas",9217.5194249482629,"Nm3/h",null,"gas",9217.5194249482629,"Nm3/h",null,"X",193.96092005269668,"g/kg"]
[null,"dry",null,null,null,null,8429.0749347470319,"kg/h",null,null,2594.8108702048812,"kg/h",null,null,11023.885804951913,"kg/h",null,null,11023.885804951913,"kg/h",null,null,11023.885804951913,"kg/h",null,null,11023.885804951913,"kg/h",null,null,11023.885804951913,"kg/h",null,"acid"]
[null,"C",38.303747534516766,"%",null,null,"Vol(wet) %",null,null,null,"Vol(wet) %",null,null,null,"Vol(wet) %",null,null,null,"Vol(wet) %",null,null,null,"Vol(wet) %",null,null,null,"Vol(wet) %",null,null,null,"Vol(wet) %",null,null,"SO2/SO3",6,"%"]
[null,"H",2.9876923076923076,"%",null,"N2",55.790646723909099,null,null,"N2",59.750222423278409,null,null,"N2",56.712794582326325,null,null,"N2",56.712794582326325,null,null,"N2",56.712794582326325,null,null,"N2",56.712794582326325,null,null,"N2",56.712794582326325,null,null,"DP",168.67817126424706,"°C"]
[null,"N",3.44,"%",null,"CO2",8.430548408165885,null,null,"CO2",6.9422658784377491,null,null,"CO2",8.0839414351694678,null,null,"CO2",8.0839414351694678,null,null,"CO2",8.0839414351694678,null,null,"CO2",8.0839414351694678,null,null,"CO2",8.0839414351694678]
[null,"O",16.968560157790929,"%",null,"H2O",30.041565778342488,null,null,"H2O",24.934563822510391,null,null,"H2O",28.85219316014674,null,null,"H2O",28.85219316014674,null,null,"H2O",28.85219316014674,null,null,"H2O",28.85219316014674,null,null,"H2O",28.85219316014674,null,null,{"$f":"AF5","v":"Link"},"Link to Gas"]
[null,"S",1,"%",null,"O2",5.5966747377326014,null,null,"O2",8.257197979523859,null,null,"O2",6.2162855233220373,null,null,"O2",6.2162855233220373,null,null,"O2",6.2162855233220373,null,null,"O2",6.2162855233220373,null,null,"O2",6.2162855233220373]
[null,"ash",36.5,"%",null,"SO2",8.1071538111432986E-2,null,null,"SO2",6.6759615803678382E-2,null,null,"SO2",7.7738426306541417E-2,null,null,"SO2",7.7738426306541417E-2,null,null,"SO2",7.7738426306541417E-2,null,null,"SO2",7.7738426306541417E-2,null,null,"SO2",7.7738426306541417E-2]
[null,"Cl",0.8,"%",null,"HCl",5.9492813738493071E-2,null,null,"HCl",4.8990280445924975E-2,null,null,"HCl",5.704687272889452E-2,null,null,"HCl",5.704687272889452E-2,null,null,"HCl",5.704687272889452E-2,null,null,"HCl",5.704687272889452E-2,null,null,"HCl",5.704687272889452E-2]
[null,"F",0,"%",null,"O2 (dry)",8,"%",null,"O2 (dry)",11,"%",null,null,"Link to R - Gas",null,null,null,0,null,null,null,0,null,null,null,0,null,null,null,0]
[null,"O/C",0.443,"(mass)",null,"Air",5018.3101289459437,"Nm3/h",null,"Air",1633.5394160591841,"Nm3/h",null,{"$f":"H5","v":"Link"},"Link to Gas"]
[null,"H/C",7.8E-2,"(mass)",null,"base",15,"°C",null,"base",15,"°C",null,{"$f":"L5","v":"Link"},"Link to Gas"]
[null,null,null,null,null,"heated",200,"°C",null,"heated",320,"°C",null,null,null,null,null,"Loss",1,"%",null,"Loss",1,"%",null,"Loss",1,"%",null,"Loss",1,"%"]
[null,null,null,null,null,"H2O",7,"g/kg",null,"H2O",7,"g/kg"]
[null,null,null,null,null,"Fuel",2400,"kg/h",null,"Fuel",{"$f":"G24/(100-J3)*J3","v":600},"kg/h",null,null,null,null,null,{"$f":"T28","v":"Link"},"Link to user",null,null,{"$f":"X28","v":"Link"},"Link to user",null,null,{"$f":"AB28","v":"Link"},"Link to user",null,null,{"$f":"AF28","v":"Link"},"Link to user"]
[null,"Emissions",null,{"$f":"_xll.alera(\"TX0218EMIS01\",C27,C28,C40,C43,C46,,,,,,,,,,,,,B49)","v":"Link"},null,"Loss",5,"%",null,"Loss",5,"%",null,null,null,null,null,{"$f":"P5","v":"Link"},"Link to Gas",null,null,{"$f":"T5","v":"Link"},"Link to Gas",null,null,{"$f":"X5","v":"Link"},"Link to Gas",null,null,{"$f":"AB5","v":"Link"},"Link to Gas"]
[null,"Basis dry gas"]
[null,"O2",11,"%",null,null,"Link to R - Gas",null,null,null,"Link to R - Gas"]
[null,"Temp",0,"°C",null,null,"Extra gas",null,null,null,"Extra gas",null,null,null,null,null,null,"Total",null,{"$f":"_xll.alera(\"TX0218APHX01\")","v":"Link"},null,"Saturated",null,{"$f":"_xll.alera(\"TX0218STEM02\",W36,,,,,,,,,,,,,,,,,,V41)","v":"Link"},null,"Total",null,{"$f":"_xll.alera(\"TX0218APHX01\")","v":"Link"},null,"H2O Heater T",null,{"$f":"_xll.alera(\"TX0218STEM08\",AE34,AE35,,,,,,,,,,,,,,,,AD41)","v":"Link"},null,"Feed Water",null,{"$f":"_xll.alera(\"TX0218STEM01\",AI32,AI34,AI35,,,,,,,,,,,,,,,,)","v":"Link"}]
[null,null,2.8260964746771338,{"$f":"_xll.aleraTX(\"TX0594TXEMIS01\")","v":"Nm3/kg"},null,{"$f":"D5","v":"Link"},"Link to Fuel",null,null,{"$f":"D5","v":"Link"},"Link to Fuel",null,null,null,null,null,null,"APH",0.18975866625070972,{"$f":"_xll.aleraTX(\"TX0554TXAPHX01\")","v":"MW net"},null,null,null,null,null,"APH",0.34495564728369432,{"$f":"_xll.aleraTX(\"TX0554TXAPHX01\")","v":"MW net"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Inlet",15,"°C",null,"Q out",2.399727270880085,{"$f":"_xll.aleraTX(\"TX0554TXSTEM02\")","v":"MW net"},null,"Inlet",15,"°C",null,"Q out",0.5449838584991199,{"$f":"_xll.aleraTX(\"TX0554TXSTEM08\")","v":"MW net"},null,"Q out",0.32556449408046728,{"$f":"_xll.aleraTX(\"TX0554TXSTEM01\")","v":"MW net"}]
[null,"Emissions",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Exit",320,"°C",null,"used",1.854743412380965,"MW",null,"Exit",200,"°C",null,"used",0.21941936441865262,"MW"]
[null,"SO2",2603.1085866735866,"mg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,"P2/P1","12,5",null,null,"Flow",3100,"kg/h",null,"P2/P1","5,7",null,null,"Flow",3100,"kg/h",null,"Flow",3100,"kg/h"]
[null,"HCl",1072.0653124009625,"mg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"L5","v":"Link"},"Comb.",null,null,"T in",150,"°C",null,{"$f":"H5","v":"Link"},"Comb.",null,null,"T in",90,"°C"]
[null,"HF",0,"mg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T exit",191.71275852521885,"°C",null,null,null,null,null,"T exit",150,"°C",null,"T exit",90,"°C"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Press.",null,null,null,null,null,null,null,"Press.",15,"bar (a)",null,"Press.",15,"bar (a)"]
[null,"Dust",47554.285992785743,"mg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"used",13,"bar (a)",null,null,null,null,null,"used",15.01,"bar (a)",null,"used",15,"bar (a)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Enth.",2786.7800565059051,"kJ/kg",null,null,null,null,null,"Enth.",632.88448083768765,"kJ/kg",null,"Enth.",378.07489635151035,"kJ/kg"]
[null,"Others"]
[null,"Fuel dry"]
[null,null,0,"mg/kg"]
[null,null,0,"mg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"AF28","v":"Link"},"Link to Boiler",null,null,null,null,null,null,{"$f":"AJ28","v":"Link"},"Link to Boiler"]
[]
[null,null,0,"mg/kg",null,null,null,null,null,null,null,null,null,null,null,null,null,"Counter Flow",null,{"$f":"_xll.alera(\"TX0218KXAX01\",,,,,,,,,,,,,,,,,,,R47,R48)","v":"Link"},null,"Counter Flow",null,{"$f":"_xll.alera(\"TX0218KXAX01\",,,,,,,,,,,,,,,,,,,V47,V48)","v":"Link"},null,"Counter Flow",null,{"$f":"_xll.alera(\"TX0218KXAX01\",,,,,,,,,,,,,,,,,,,Z47,Z48)","v":"Link"},null,"Counter Flow",null,{"$f":"_xll.alera(\"TX0218KXAX01\",,,,,,,,,,,,,,,,,,,AD47,AD48)","v":"Link"}]
[null,null,0,"mg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,"dTLog",586.18488646749222,{"$f":"_xll.aleraTX(\"TX0558TXKXAX01\")","v":"°C"},null,"dTLog",306.08718821465436,{"$f":"_xll.aleraTX(\"TX0558TXKXAX01\")","v":"°C"},null,"dTLog",183.93428813124356,{"$f":"_xll.aleraTX(\"TX0558TXKXAX01\")","v":"°C"},null,"dTLog",105.45197402268913,{"$f":"_xll.aleraTX(\"TX0558TXKXAX01\")","v":"°C"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"K x A",323.71811459392359,null,null,"K x A",6059.5264480010228,null,null,"K x A",1875.4287239666612,null,null,"K x A",2080.7516070912257]
[null,null,0,"mg/kg"]
[null,null,0,"mg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"T28","v":"Link"},"Exchanger 1",null,null,{"$f":"X5","v":"Link"},"Exchanger 1",null,null,{"$f":"AB28","v":"Link"},"Exchanger 1",null,null,{"$f":"AF5","v":"Link"},"Exchanger 1"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"T5","v":"Link"},"Exchanger 2",null,null,{"$f":"X28","v":"Link"},"Exchanger 2",null,null,{"$f":"AB5","v":"Link"},"Exchanger 2",null,null,{"$f":"AF28","v":"Link"},"Exchanger 2"]
[null,{"$f":"D5","v":"Link"},"Link to Fuel"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"K",40,"W/m2K",null,"K",80,"W/m2K",null,"K",40,"W/m2K",null,"K",80,"W/m2K"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"area",{"$f":"S29*1000000/S51/S44","v":8.0929528648480886},"m2",null,"area",{"$f":"W30*1000000/W51/W44","v":98.000151724628537},"m2",null,"area",{"$f":"AA29*1000000/AA51/AA44","v":46.885718099166525},"m2",null,"area",{"$f":"AE30*1000000/AE51/AE44","v":64.600955025965277},"m2"]