{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":1,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":25,"n_cols":31,"rows_kept":25,"cut":false,"hidden":false,"merged":[]}
[]
[null,"(mass) Analysis Axis",1.327,{"$f":"0.334*4.5/4","v":0.37575000000000003}]
[null,null,"X","Y"]
[null,null,"atomic O/C","atomic H/C",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fuel",null,{"$f":"_xll.alera(\"TX0218FUEL01\",AD6,AD13,AD15,AD16,AD17,AD18,AD19,AD20)","v":"Link"}]
[null,"Proteine",0.3,1.65,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F00000000"]
[null,"Wood",0.68,1.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"H2O",3,"%"]
[null,"Crude Oil",0.02,2]
[null,"Methane",0,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LCV",17.501744631400001,{"$f":"_xll.aleraTX(\"TX0550TXFUELBX\")","v":"MJ/kg"}]
[null,"Sewage Sludge",0.45,1.6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"G 6"]
[null,"Black Liquor (Mg)",0.75,1.45,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dry"]
[null,"Asphalte",0.02,1.3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"C",48.04,"%"]
[null,"Propane",0,2.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"H",6,"%"]
[null,"Formaldehyde",1,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N",1,"%"]
[null,"Ethanol",0.5,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"O",42.76,"%"]
[null,"Peat",0.5,1.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S",0.2,"%"]
[null,"Lignine",0.41,1.3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ash",2,"%"]
[null,"Lignite",0.3,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cl",0,"%"]
[null,"Subbituminous",0.18,0.9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F",0,"%"]
[null,"Bituminous",0.05,0.65,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"O/C",0.89009159034138219,"(mass)"]
[null,"Anthracite",2.5000000000000001E-2,0.3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"H/C",0.12489592006661115,"(mass)"]
[null,"Your Fuel atomic",0.6,2.2000000000000002]
[]
[null,null,"O/C","H/C"]
[null,null,"Analysis (m)","Analysis (m)"]
[null,"Your Fuel Analytic",0.89,0.125]